# These constants are taken from "DPU Table Generation tasks in "PLASTIC IDPU Software Requirements"				
A1	4.91159	  # used for finding ln(M)		
A2	-1.40138  # used for finding ln(M)			
A3	-2.81478  # used for finding ln(M)			
A4	0.472268  # used for finding ln(M)			
A5	0.080699  # used for finding ln(M)			
A6	0.077267 # used for finding ln(M)			
Ae	2	  # Emeas = Eun * A + B		
At	0.25	  # Tns = Tch * A + B		
Be	0	  # Emeas = Eun * A + B		
Bt	1.3	  # Tns = Tch * A + B		
C2	2			# M/q = C1 * [PAC + (E/q)-C2]*Tns^2
d_nossd	5.8			# C1 = f(d) -- d = flight path in cm (but not in SSD)
d_ssd	8			# C1 = f(d) -- d = flight path in cm (but not in SSD)
D1	0.2		# E/q = D1 * D2^S	
D2	1.048954346     # E/q = D1 * D2^S			
Emax	2010	      # keV -- for binning Nm		
Emin	15	      # keV -- for binning Nm		
Mmax	95	      # for finding the bins for Mass		
Mmin	0.5	      # for finding the bins for Mass		
MQmax	60	      # for finding the bins for Mass/Charge		
MQmin	0.5	      # for finding the bins for Mass/Charge		
NMAX	90	      # for finding the bins for Mass		
NQMAX	254	      # for finding the bins for Mass/Charge		
Tmax	250.5	      # nsec -- for binning Nm		
Tmin	6	      # nsec -- for binning Nm		
